# Siebel Center 4403



## Turning the System On

* Press the power button once.
* The buttons will flash for approximately 30 seconds as the projector starts up. You may now select a source (The Apple TV is the default source).

Note: The system must be turned on before sources can be selected.

## Using a Laptop

* Connect your laptop to the end of the VGA cable that is not connect to the input panel.
* Select the [Computer] button on the control panel.

Control Panel

Note: The input panel on this system has two VGA ports. One is labeled **[Input]** and the other is labeled **[Monitor]**. Ensure the VGA cable is plugged into the **[Input]** port.

## Using a Composite Video Device

* Connect an RCA cable (user provided) between your device and the composite video ports on the input panel.
* Select the [Composite Video] button on the control panel.

## Turning the System Off

* Press and hold the power button for 6 seconds.
* The buttons will flash for 30-90 seconds as the system shuts down.